{"text_format":"3","workbook":"xls","n_sheets":6,"sheets":["目录及联系方式","字符点阵","图形点阵","中文图形两用型","TFT彩屏","OLED屏"],"not_rendered":{"images":1,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"目录及联系方式","index":0,"n_rows":11,"n_cols":2,"rows_kept":11,"merged":[[0,0,0,1],[1,0,1,1],[10,0,14,0],[10,1,14,1]],"flags":["formulas_cached_only"]}
["肇庆市金鹏实业有限公司"]
[]
["产品类型","点击查看"]
["字符点阵单色屏",1]
["图形点阵单色屏（SMT、COB、COG）\n（可带触摸屏）",2]
["中文图形两用型单色屏（SMT、COB、TAB）\n（可带触摸屏）",3]
["TFT彩屏\n（可带触摸屏,部分可选电容触摸屏）",4]
["OLED屏",5]
["公司官网","http://www.gptlcm.cn"]
["官方淘宝店","https://shop557780818.taobao.com/?spm=a230r.7195193.1997079397.2.1b4d39f88jNr9n"]
["官方微信公众号"]

{"sheet":"字符点阵","index":1,"n_rows":11,"n_cols":6,"rows_kept":11,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
[" 液晶显示模块 -> 字符点阵"]
["型  号","显示点阵","模块尺寸","视域尺寸","控制芯片","网站及资料链接"]
["OCMC1X16A","1行X16字符","80X36X13","64.3X13.8","ST7066或兼容","下载"]
["OCMC2X16A","2行X16字符","80X36X13","64.3X13.8","ST7066或兼容","下载"]
["OCMC2X16B","2行X16字符","122X44X13.5","99X24","ST7066或兼容","下载"]
["OCMC2X20","2行X20字符","116X37X13.5","83X18.5","ST7066或兼容","下载"]
["OCMC2X40","2行X40字符","182X33.5X11","154X15.8","NT7070/\nST7066或兼容","下载"]
["OCMC1604-2","4行X16字符","75X55X13","62X25.5","NT7070/\nST7066或兼容","下载"]
["OCMC4X20","4行X20字符","98X60X14","76X25.9","NT7070/\nST7066或兼容","下载"]
[]
[null,null,"回目录"]

{"sheet":"图形点阵","index":2,"n_rows":34,"n_cols":13,"rows_kept":34,"merged":[[0,0,0,4],[0,7,0,11]],"flags":["formulas_cached_only"]}
[" 液晶显示模块 -> 图形点阵",{"$nulls":6},"  触摸屏液晶显示模块 -> 图形点阵"]
["型  号","显示点阵","模块尺寸","视域尺寸","控制芯片","网站及资料链接",null,"型  号","显示点阵","模块尺寸","视域尺寸","控制芯片","网站及资料链接"]
["OCM12232-1","122X32点阵","84X44X13","60X18","SED1520\\\nSBN1661或兼容","下载",null,"OCM240128-1","240X128点阵","144X104X18.8","114X64","T6963C\\\nRA6963或兼容","下载"]
["OCM12232-2","122X32点阵","84X44X13","60X18","SED1520\\\nSBN1661或兼容","下载",null,"OCM240128-2","240X128点阵","144X104X15","114X64","T6963C\\\nRA6963或兼容","下载"]
["OCM12232-3","122X32点阵","84X44X13","60X18","SED1520\\\nSBN1661或兼容","下载",null,"OCM320240-3","320X240点阵","160X109X12","121X93","RA8835","下载"]
["OCM12232-5","122X32点阵","84X44X13","60X18","SED1520\\\nSBN1661或兼容","下载"]
["OCM12232-6","122X32点阵","80.9X29X13","60X18","SED1520\\\nSBN1661或兼容","下载"]
["OCM12832-1","128X32点阵","110X65X13.5","77.5X24.3","KS0108\\\nAIP31108或兼容","下载"]
["OCM12864-1","128X64点阵","113X65X12.5","73.4X38.8","KS0108\\\nAIP31108或兼容","下载"]
["OCM12864-2","128X64点阵","93X70X13.5","70.5X38.5","KS0108\\\nAIP31108或兼容","下载"]
["OCM12864-3","128X64点阵","78X70X12","62X44","KS0108\\\nAIP31108或兼容","下载"]
["OCM12864-4","128X64点阵","78X70X12","62X44","T6963C\\\nRA6963或兼容","下载"]
["OCM12864-5","128X64点阵","54X50X8.7","43.5X29","KS0108\\\nAIP31108或兼容","下载"]
["OCM19264-1","192X64点阵","130X65X12.5","104X38.5","KS0108\\\nAIP31108或兼容","下载"]
["OCM19264-2","192X64点阵","100X60X12.5","84X31","KS0108\\\nAIP31108或兼容","下载"]
["OCM19264-2A","192X64点阵","100X60X12.5","84X31","KS0108\\\nAIP31108或兼容","下载"]
["OCM19264-3","192X64点阵","113X71X12","97X48","KS0108\\\nAIP31108或兼容","下载"]
["OCM25664-1","256X64点阵","137X39.6X10.6","108X32","KS0108\\\nAIP31108或兼容","下载"]
["OCM128128","128X128点阵","99X100X17","69X69","T6963C\\\nRA6963或兼容","下载"]
["OCM160128-1","160X128点阵","129X102X12.5/17","101X82","T6963C\\\nRA6963或兼容","下载"]
["OCM24064-1","240X64点阵","180X65X13.5","132X39","T6963C\\\nRA6963或兼容","下载"]
["OCM240128-1","240X128点阵","144X104X18.8","114X64","T6963C\\\nRA6963或兼容","下载"]
["OCM240128-2","240X128点阵","144X104X15","114X64","T6963C\\\nRA6963或兼容","下载"]
["OCM240128-3","240X128点阵","144X104X15","114X64","T6963C\\\nRA6963或兼容","下载"]
["OCM240128-7","240X128点阵","120X73X12.5","93X48","T6963C\\\nRA6963或兼容","下载"]
["OCM320240-3","320X240点阵","160X109X12","121X93","RA8835","下载"]
["OCM320240-6","320X240点阵","139X107X13.8","103X79","RA8835","下载"]
["OCMJ320240B","320X240点阵","160X169X13.8 ","121×93","LPC2136","下载"]
["OCM12864-8","128X64点阵","92X53X8.5","65.3X37.5","ST7565","下载"]
["OCM12864-9","128X64点阵","42X37X7","30X22","ST7565","下载"]
["OCM128128-2","128X128点阵","65X66.5X7","48.78X48.78","ST7541","下载"]
[]
[]
[null,null,"回目录"]

{"sheet":"中文图形两用型","index":3,"n_rows":45,"n_cols":13,"rows_kept":45,"merged":[[0,0,0,4],[0,7,0,11],[5,11,6,11],[7,7,8,7],[7,8,8,8],[7,10,8,10]],"flags":["formulas_cached_only"]}
[" 液晶显示模块 -> 中文图形两用型",{"$nulls":6},"  触摸屏液晶显示模块 -> 中文图形两用型"]
["型  号","显示点阵","模块尺寸","视域尺寸","控制芯片","网站及资料链接",null,"型  号","显示点阵","模块尺寸","视域尺寸","控制芯片","网站及资料链接"]
["OCMJ2X8A","2行X8中文 128X32点阵","110X65X13.5","77.5X24.5","GPL133A","下载",null,"OCMJ8X15D","8行X15中文 240X128点阵","144X104X14","114X64","RA8822/RA8806","下载"]
["OCMJ4X8B-1","4行X8中文 128X64点阵","93.5X73.4X13.6","70.5X38.5","GPL133A","下载",null,"OCMJ15X20D","15行X20中文 320X240点阵","167X109X14","121X92","RA8803/RA8806","下载"]
["OCMJ4X8B-2","4行X8中文 128X64点阵","110X70X13.6","70.5X38.5","GPL133A","下载",{"$nulls":3},"回目录"]
["OCMJ4X8B-3","4行X8中文 128X64点阵","78X70X12.5","62X44","GPL133A","下载"]
["OCMJ4X12B","4行X12中文 192X64点阵","130X65X12.5 ","104×38.5","GPL133A","下载"]
["OCMJ5X10B","5行X10中文 160X80点阵","122.4X80X12.2","88X46.5","GPL133A","下载"]
["OCMJ8X8B","8行X8中文 128X128点阵","99X100X14","69×69","GPL133A","下载"]
["OCMJ8X10B","8行X10中文 160X128点阵","129X102X16.8","101X82","GPL133A","下载"]
["OCMJ8X15B","8行X15中文 240X128点阵","144X104X14.5","114X64","GPL133A","下载"]
["OCMJ12232C-1","2行X7.5中文 122X32点阵","84X44X13","60X18","ST7920","下载"]
["OCMJ12232C-2","2行X7.5中文 122X32点阵","81X44X13","60X18","ST7920","下载"]
["OCMJ12232C-3","2行X7.5中文 122X32点阵","70X34X11","58X20","ST7920","下载"]
["OCMJ12232C-4","2行X7.5中文 122X32点阵","76.8X28X12","61×19","ST7920","下载"]
["OCMJ2X4C","2行X4中文 64X32点阵","58X32X12","38×16","ST7920","下载"]
["OCMJ2X8C","2行X8中文 128X32点阵","84X44X14.2","70X20","ST7920","下载"]
["OCMJ2X8C-2","2行X8中文 128X32点阵","110X65X13.5","77.5X24.5","ST7920","下载"]
["OCMJ2X8C-4","2行X8中文 128X32点阵","87X40X14.2","70X20","ST7920","下载"]
["OCMJ2X8C-5","2行X8中文 128X32点阵","65X38X12.3","53.8X15.2","ST7920","下载"]
["OCMJ2X8C-7","2行X8中文 128X32点阵","80X42.8X13","60X14.36","ST7920","下载"]
["OCMJ2X10C","2行X10中文 160X32点阵","116X39X13","85.8X19.2","ST7920","下载"]
["OCMJ2X10C-2","2行X10中文 160X32点阵","122X44X13","99X24","ST7920","下载"]
["OCMJ2X10C-5","2行X10中文 160X32点阵","122X32X14","92X22","ST7920","下载"]
["OCMJ4X8C","4行X8中文 128X64点阵","93X70X13 ","73X39","ST7920","下载"]
["OCMJ4X8C-3","4行X8中文 128X64点阵","88X70X13","73X39","ST7920","下载"]
["OCMJ4X8C-4","4行X8中文 128X64点阵","80X80X13","73X39","ST7920","下载"]
["OCMJ4X8C-6","4行X8中文 128X64点阵","93X65X13","73X39","ST7920","下载"]
["OCMJ4X8C-7","4行X8中文 128X64点阵","83X66X13","73X39","ST7920","下载"]
["OCMJ4X8C-8","4行X8中文 128X64点阵","78X70X12","62X44","ST7920","下载"]
["OCMJ4X8C-14","4行X8中文 128X64点阵","75X61.5X13","55X38","ST7920","下载"]
["OCMJ4X8C-15","4行X8中文 128X64点阵","80.5X71.6X13","65X50","ST7920","下载"]
["OCMJ4X8C-16","4行X8中文 128X64点阵","75X52.7X8.9","60X32.6","ST7920","下载"]
["OCMJ4X4C","4行X4中文 64X60点阵","67X53X12","48.6X30","ST7920","下载"]
["OCMJ4X12C","4行X12中文 192X64点阵","130.4X65X12.5","104X39","ST7920","下载"]
["OCMJ4X16C","4行X16中文 256X64点阵","145.34X66.5X12.5","104X38.5","ST7920","下载"]
["OCMJ4X16A","4行X16中文 256X64点阵","180X65X12","131.5X38.8","ST7920","下载"]
["OCMJ4X16A-3","4行X16中文 256X64点阵","180X65X12","131.5X38.8","ST7920","下载"]
["OCMJ8X10D","8行X10中文 160X128点阵","129X102X17.2","101X82","RA8822/RA8806","下载"]
["OCMJ5X10D","5行X10中文 160X80点阵","122.4X80X14.8","88X46.5","RA8822/RA8806","下载"]
["OCMJ8X15D","8行X15中文 240X128点阵","144X104X14","114X64","RA8822/RA8806","下载"]
["OCMJ8X15D-2","8行X15中文 240X128点阵","120X73X12.6","93X48","RA8822/RA8806","下载"]
["OCMJ15X20D","15行X20中文 320X240点阵","167X109X14","121X92","RA8803/RA8806","下载"]
[]
[null,null,"回目录"]

{"sheet":"TFT彩屏","index":4,"n_rows":52,"n_cols":12,"rows_kept":52,"merged":[[0,0,0,11],[2,0,2,11],[3,0,15,0],[3,11,15,11],[16,0,16,11],[17,0,29,0],[17,11,29,11],[30,0,30,11],[31,0,43,0],[31,11,43,11],[44,0,44,11],[45,0,47,0],[45,11,47,11],[48,0,48,11],[49,0,50,0]],"flags":["formulas_cached_only"]}
[" 液晶显示模块 ->  TFT彩屏(彩屏可按客户要求加带触摸屏)"]
[null,null,"型  号","分辨率","模块尺寸","视域尺寸","工作电压","接口类型","触摸屏类型","串口通讯电平","网站及资料链接","产品特点"]
["UART串口屏产品（带上位机开发软件）"]
["5D","3.5寸","OCM320240T350-5D","320X240","96X70X12.6","72.4X54.6(3.5寸)","5-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载","5D系列产品，国产芯片架构，可选配全国产材料，128M bit的存储容量。\n\n其他特点：\n(1) 基于寄存器(即变量)工作，某种类型控件只是变量的一种表现形式。\n(2) 用户可以通过“金鹏终端开发软件”轻松设计出千变万化炫丽的GUI 界面而无需写任何代码；\n(3) 基于相同寄存器的不同控件是相互联动的，只要寄存器的数值发生了变化，所有相关联的控件都将相应发生变化。\n(4) 大大缩短开发周期，产品升级非常便利。\n"]
[null,"3.5寸","OCM320480T350-5D","320X480","96X60","74.6X50.2(3.5寸)","5-24V","串口(UART)","电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.0寸","OCM480480T400-5D","480X480","96X70X12.7","72.1X70.4(4寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.3寸","OCM480272T430-5D","480X272","119.76X72.71X13.8","97.9X56.7(4.3寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.3寸","OCM800480T430-5D","800X480","119.76X72.71X13.8","97.9X56.7(4.3寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"5.0寸","OCM800480T500-5D","800X480","143.47X81X10.1","109.6X66.4(5寸)","5/7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"5.6寸","OCM640480T560-5D","640X480","146X110X16.5","115.3X87.1(5.6寸)","5/7.6-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"6.2寸","OCM800480T620-5D","800X480","179X97X16.5","139.7X79.7(6.2寸)","5/7.6-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"7.0寸","OCM800480T700-5D","800X480","189X110.3X17","156.7X89.1(7寸)","5/7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"7.0寸","OCM1024600T700-5D","1024X600","189X110.3X17","156.7X89.1(7寸)","5/7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"8.0寸","OCM800600T800-5D","800X600","199.4X148.8X18","163.6X123.4(8寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"10.1寸","OCM1024600T101-5D","1024X600","257.81X148.08X16.1","224.7X127.28(10.1寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"10.4寸","OCM800600T104-5D","800X600","247.8X193.7X17.5","212.8X160(10.4寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[]
["4D","3.5寸","OCM320240T350-4D","320X240","96X70X12.6","72.4X54.6(3.5寸)","5-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载","4D系列产品，进口芯片架构，128M bit的存储容量。\n\n其他特点：\n(1) 基于寄存器(即变量)工作，某种类型控件只是变量的一种表现形式。\n(2) 用户可以通过“金鹏终端开发软件”轻松设计出千变万化炫丽的GUI 界面而无需写任何代码；\n(3) 基于相同寄存器的不同控件是相互联动的，只要寄存器的数值发生了变化，所有相关联的控件都将相应发生变化。\n(4) 大大缩短开发周期，产品升级非常便利。\n"]
[null,"3.5寸","OCM320480T350-4D","320X480","96X60","74.6X50.2(3.5寸)","5-24V","串口(UART)","电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.0寸","OCM480480T400-4D","480X480","96X70X12.7","72.1X70.4(4寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.3寸","OCM480272T430-4D","480X272","119.76X72.71X13.8","97.9X56.7(4.3寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.3寸","OCM800480T430-4D","800X480","119.76X72.71X13.8","97.9X56.7(4.3寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"5.0寸","OCM800480T500-4D","800X480","143.47X81X10.1","109.6X66.4(5寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"5.6寸","OCM640480T560-4D","640X480","146X110X16.5","115.3X87.1(5.6寸)","5/7.6-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"6.2寸","OCM800480T620-4D","800X480","179X97X16.5","139.7X79.7(6.2寸)","5/7.6-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"7.0寸","OCM800480T700-4D","800X480","189X110.3X17","156.7X89.1(7寸)","5/7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"7.0寸","OCM1024600T700-4D","1024X600","189X110.3X17","156.7X89.1(7寸)","5/7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"8.0寸","OCM800600T800-4D","800X600","199.4X148.8X18","163.6X123.4(8寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"10.1寸","OCM1024600T101-4D","1024X600","257.81X148.08X16.1","224.7X127.28(10.1寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"10.4寸","OCM800600T104-4D","800X600","247.8X193.7X17.5","212.8X160(10.4寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[]
["3D","3.5寸","OCM320240T350-3D","320X240","96X70X12.6","72.4X54.6(3.5寸)","5-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载","3D系列产品，进口芯片架构，1G bit的存储容量。\n\n其他特点：\n(1) 基于寄存器(即变量)工作，某种类型控件只是变量的一种表现形式。\n(2) 用户可以通过“金鹏终端开发软件”轻松设计出千变万化炫丽的GUI 界面而无需写任何代码；\n(3) 基于相同寄存器的不同控件是相互联动的，只要寄存器的数值发生了变化，所有相关联的控件都将相应发生变化。\n(4) 大大缩短开发周期，产品升级非常便利。\n"]
[null,"3.5寸","OCM320480T350-3D","320X480","96X60","74.6X50.2(3.5寸)","5-24V","串口(UART)","电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.0寸","OCM480480T400-3D","480X480","96X70X12.7","72.1X70.4(4寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.3寸","OCM480272T430-3D","480X272","119.76X72.71X13.8","97.9X56.7(4.3寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"4.3寸","OCM800480T430-3D","800X480","119.76X72.71X13.8","97.9X56.7(4.3寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"5.0寸","OCM800480T500-3D","800X480","143.47X81X10.1","109.6X66.4(5寸)","5-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"5.6寸","OCM640480T560-3D","640X480","146X110X16.5","115.3X87.1(5.6寸)","5/7.6-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"6.2寸","OCM800480T620-3D","800X480","179X97X16.5","139.7X79.7(6.2寸)","5/7.6-24V","串口(UART)","电阻屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"7.0寸","OCM800480T700-3D","800X480","189X110.3X17","156.7X89.1(7寸)","5/7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"7.0寸","OCM1024600T700-3D","1024X600","189X110.3X17","156.7X89.1(7寸)","5/7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"8.0寸","OCM800600T800-3D","800X600","199.4X148.8X18","163.6X123.4(8寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"10.1寸","OCM1024600T101-3D","1024X600","257.81X148.08X16.1","224.7X127.28(10.1寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
[null,"10.4寸","OCM800600T104-3D","800X600","247.8X193.7X17.5","212.8X160(10.4寸)","7.6-24V","串口(UART)","电阻屏/电容屏","(非标232-TTL)/RS232/RS485","下载"]
["（三线/四线)SPI串口/（8位/16位）并口液晶屏产品（自行切换接口、无上位机开发软件）"]
["B     系       列","3.5寸","OCM320240T350-5B","320X240","93X70X16.6","72.4X54.6(3.5寸)","5V","串并可选","电阻屏",null,"下载","5B系列产品，带图片预存功能和串并可选功能"]
[null,"4.3寸","OCM480272T430-5B","480X272","127X88X16.8","97.9X56.7(4.3寸)","5V","串并可选","电阻屏",null,"下载"]
[null,"7.0寸","OCM800480T700-5B","800X480","178.7X110.6X17.3","154.08X85.92(7寸)","5/7.6-24V","串并可选","电阻屏",null,"下载"]
["小尺寸串口液晶屏产品"]
[null,"1.44寸","GP-SX-128128T1.44-SPI","128X128","45.5X29.7","26.5X25.5(1.44寸)","3.3V","串口(4线SPI)","无",null,"下载","四线SPI串口的液晶屏产品"]
[null,"2.8寸","OCM320240T280-2A","320X240","84.0X56.3(V1.X)\n84.0X65.6(V2.x)(V3.x)","57.6X43.2(2.8寸)","3.3/5V","串口(UART)","电阻屏",null,"下载","UART串口液晶屏产品（配套上位机下载图片字库）"]
[{"$nulls":5},"回目录"]

{"sheet":"OLED屏","index":5,"n_rows":21,"n_cols":12,"rows_kept":21,"merged":[[0,0,0,11]],"flags":["formulas_cached_only"]}
[" OLED显示模块 -> OLED显示模块"]
[" 显示尺寸 /英寸","型  号","显示点阵","模块尺寸","视域尺寸","点尺寸","控制芯片","封装","接口方式","工作电压(V)","屏颜色","网站及资料链接"]
["2.7寸","OCMO12864-1","128X64点阵","74X56.5X5.8","63.41X32.69","0.45X0.45","SSD1325","TAB","并口/串口","3.3V","黑底白//黄字","下载"]
["0.96寸","OCMO12864-2","128X64点阵","32X30X4.2","23.74X12.86","0.154X0.154","SSD1306","COG","并口/串口","3.3V/5V"," 黑底白/蓝字/黄蓝双色","下载"]
["1.3寸","OCMO12864-3","128X64点阵","34.5X35X4.2","31.42X16.7","0.21X0.21","SSD1306","COG","并口/串口","3.3V/5V","黑底白字","下载"]
["1.54寸","OCMO12864-4","128X64点阵","46X44X5.1","37.05X19.52","0.254X0.254","SSD1309","COG","并口/串口","3.3V/5V","黑底白/黄/蓝","下载"]
["2.42寸","OCMO12864-5","128X64点阵","66X53X5.5","57.01X29.49","0.4.X0.40","SSD1309","COG","并口/串口","3.3V/5V","黑底白/黄/蓝","下载"]
["2.23寸","OCMO12832-1","128X32点阵","66X41.5X6.4","57.02×15.1","0.41X0.39","SSD1309","COG","并口/串口","3.3V/5V","黑底白/蓝字","下载"]
["5.5寸","OCMO25664-1","256X64点阵","159.33X49.8X6.5","137.65x35.89","0.5X0.5","SSD1322","TAB","并口/串口","3.3V/5V","黑底绿字","下载"]
["2.8寸","OCMO25664-2","256X64点阵","103X33.5X6.5","71.104X19.264","0.254X0.254","SSD1322","TAB","并口/串口","3.3V/5V","黑底蓝字","下载"]
["3.12寸","OCMO25664-3","256X64点阵","103X33.5X6.5","78.78X21.18","0.28X0.28","SSD1322","TAB","并口/串口","3.3V/5V","黑底白/蓝字","下载"]
["2.7寸","OCMO12864-1A","128X64点阵","93X70X7.5","63.41X32.69","0.45X0.45","SSD1325","TAB","并口/串口","3.3V/5V","黑底白/黄字","下载"]
["2.23寸","OCMO12832-1A","128X32点阵","66×41.5×6.4","57.02×15.1","0.41×0.39","STM8S","COG","并口/串口","3.3V/5V","黑底白/蓝字","下载"]
["0.96寸","OCMO12864-2A","128X64点阵","34.5×35×4.2","23.74×12.86","0.154×0.154","STM8S","COG","并口/串口","3.3V/5V","黑底白/蓝字/黄蓝双色","下载"]
["1.3寸","OCMO12864-3A","128X64点阵","34.5×35×4.2","31.42×16.7","0.21×0.21","STM8S","COG","并口/串口","3.3V/5V","黑底白/蓝字","下载"]
["1.54寸","OCMO12864-4A","128X64点阵","46×44×5.1","37.05×19.52","0.254×0.254","STM8S","COG","并口/串口","3.3V/5V","黑底白/黄/蓝","下载"]
["2.42寸","OCMO12864-5A","128X64点阵","66.0x53.0x5.5","57.0x29.49","0.40x0.40","STM8S","COG","并口/串口","3.3V/5V","黑底白/蓝/黄/绿字","下载"]
["5.5寸","OCMO25664-1A","256X64点阵","159.33x49.8x6.0","137.65x35.89","0.5x0.5","STM32","TAB","并口/串口","3.3V/5V","黑底绿字","下载"]
["2.8寸","OCMO25664-2A","256X64点阵","103x33.5x6.0","71.104x19.264","0.254x0.254","STM32","TAB","并口/串口","3.3V/5V","黑底蓝字","下载"]
["3.12寸","OCMO25664-3A","256X64点阵","103x33.5x6.0","78.78x21.18","0.28x0.28","STM32","TAB","并口/串口","3.3V/5V","黑底白/蓝字","下载"]
[{"$nulls":4},"回目录"]